Hi Stefan,

Yes the current draw by the freq gen is 12V 0.5 Amps its from 12 Volt 10 Amp DC converter that I use. The current reading you see is the input draw to the freq gen from the DC converter. Everything you need to make this unit is in the updated D14.pdf in the link below

http://panaceauniversity.org/D14.pdf

including the inductors....which are very very important. Then comes the conditioning which is crucial....how to is posted on oupower. Its a specific procedure that has to be followed!

Dave who was the first to replicate stan meyer system had got outputs in the range of 250% OU (without the inductors, should be more now...he hasnt talked about the outputs with the inductors). I have made my system based on his inputs and all these inputs on how you can get these kind of outputs are already posted on the oupower forum and partially here.

No I dont have a scope. My system was slightly modified and I have so many leads going in as I can control the number of tubes that can be operated without opening the WFC. I have 18 leads coming out of the WFC 9 +ve and 9 -ve.....with this I can run on one tube or six like daves or all 9....you basically have an easier control on the number of tubes to be used for experimentation without dismantling the WFC. Dave's and Stanleys systems had a spacing of 1/16" (1.5875mm) and my pipes have a gap of less than 0.670mm (could be the main reason for the higher efficiency in my unit) and im using 9 tube sets of 9" length and the inner being 1/2" more than the outer for connections. Dave used 6 tubes of 5" length for his 250% OU. Stans were 9 tubes of 18" length on his demonstration electrolyzer and in one of the videos available, there are claims that he's making 1700% OU over Faradays. When compared to this efficiency I still have some more work to do. Dave's electrolyzer generating HHO with inductors as per the updated D14..... video link...


http://www.youtube.com/watch?v=OiA4z_Kpgg4


Stefan the excess gas outputs were documented quite sometime ago by Dave. There are a few people who have connected the D14 system to vehicles.....here's a link....this guy claims his mileage increased from 28 miles/gal to 45 miles/gal....thats an increase of 17 miles per gallon.....he's even showing you how you can tune a WFC with an AM Radio!!...

http://www.youtube.com/watch?v=9fFp3CJZMTw


Everything you need to make this system is in D14 and the data which is required to make this system efficient and how to go about it has been posted by me on the oupower and here. You get very very low gas generation in the beginning when you are conditioning like you see in the pictures above and below. I dont know why it works the way it works or the theory behind why or how it works.......it just works!......Make it follow the procedure and you will achieve OU over fardays!!! I've put in efforts without thinking it would fail and it didnt...

Im posting a few pictures of WFC under construction and progress....

The wall thickness of both the pipes is 14 SWG or 2.032 mm

Ravi